IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2018-08-06T23:19:14"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150220_1215(x64) - Exporter 16.6.0.0 - Alternate UI 16.6.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "cjl@convergo.se" of Organization (no name given)
  Owner history of Person "cjl@convergo.se" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 30.344238″ | longitude -71° 3′ 35.194702″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "<Default>"
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "6661F Shower panel, 6V" | object type "6661F Shower panel, 6V" | names: "6661F:6661F Shower panel, 6V:323723" | material: materials ("Fine Textured - Black", "Aluminum - Polished") | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "6661F Shower panel, 6V" | FAUCET | 1 occurrence | material: materials ("Fine Textured - Black", "Aluminum - Polished") | property sets: Dimensions(Type), Electrical(Type), General(Type), Green Building Properties(Type), Identity Data(Type), Materials and Finishes(Type)

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other(Type) | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Oras" (IFCTEXT)
    Category = "Bathroom, shower, public & semi-public" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Aluminum/Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "6661F" (IFCTEXT)
    Features = "Battery-operated, touchless" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Aluminium" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "6661F" (IFCTEXT)
    Name = "6661F Shower panel, 6V" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "260x200x1236 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "https://warranty.oras.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Identity Data(Type) | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Class = "Battery-operated, touchless" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Group = "Shower faucets" (IFCTEXT)
    Manufacturer = "Oras" (IFCTEXT)
    Market = "INT;DNK;EST;FIN;LVA;LTU;NOR;POL;RUS;UKR" (IFCTEXT)
    Model = "6661F Shower panel, 6V" (IFCTEXT)
    Name_en = "6661F Shower panel, 6V" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "6661F" (IFCTEXT)
    Product Datasheet = "https://www.oras.com/datasheet/6661F/en" (IFCTEXT)
    Product Family = "Oras Electra" (IFCTEXT)
    Product URL = "https://www.oras.com/en/products/oras/product/6661F" (IFCTEXT)
    Type Name = "6661F Shower panel, 6V" (IFCTEXT)
    URL = "" (IFCTEXT)
    Usage Group = "Shower facilities (public saunas, swimming baths)" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Oras" (IFCLABEL)
    ModelReference = "6661F" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "6661F Shower panel, 6V" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.613833132025395 (IFCAREAMEASURE) [SQUARE_METRE]
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Volume = 0.0626703744191486 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "7" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "6661F: 6661F Shower panel, 6V" (IFCLABEL)
    Family and Type = "6661F: 6661F Shower panel, 6V" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "6661F: 6661F Shower panel, 6V" (IFCLABEL)
    Type Id = "6661F: 6661F Shower panel, 6V" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions(Type) | properties | on 1 type object
    NominalDepth = 196.5 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 1236. (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 258.2 (IFCLENGTHMEASURE) [MILLI METRE]
  Electrical(Type) | properties | on 1 type object
    Battery = "Lithium 2CR5 6 V" (IFCTEXT)
    Operating Voltage = 6. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General(Type) | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "6661F" (IFCTEXT)
    ConvergoRefNr = "0087-1809-0081-FI" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for baths" (IFCTEXT)
    NBSReference = "45-35-70/315" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_81" (IFCTEXT)
    Uniclass2015Description = "Shower thermostatic water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_81" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "27/07/2018" (IFCTEXT)
  Green Building Properties(Type) | properties | on 1 type object
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    EAN Number = "6414150047312" (IFCTEXT)
    EMC Directive = "89/336/EEC" (IFCTEXT)
    EN Standard = "EN 15091" (IFCTEXT)
    ETA-Danmark = "VA 1.41/19333" (IFCTEXT)
    LVI Number = "6319410" (IFCTEXT)
    NRF Number = "4203149" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    STF Certificate = "STF VTT-RTH-00114-11" (IFCTEXT)
    VVS Number = "723922004" (IFCTEXT)
  Materials and Finishes(Type) | properties | on 1 type object
    FaucetMainMaterial = "Aluminum - Polished" (IFCLABEL)
  Mechanical(Type) | properties | on 1 type object
    Advanced Features = "Adjustable settings (with magnetic key)" (IFCTEXT)
    Afterflow Period = 5. (IFCREAL)
    Connection Size = "G3/4" (IFCTEXT)
    Flow Rate At 300kPa = 0.00776922667872749 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Flow Rate At 300kPa With Flow Controller = 0.00706293334429772 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Wall-mounted" (IFCTEXT)
    Installation Width = "CC 150" (IFCTEXT)
    Installation and Maintenance = "https://www.oras.com/fileadmin/resources/110361_PDM_945966_8_(945966-04-15).pdf" (IFCTEXT)
    Max Flow Period = 300. (IFCREAL)
    Max. Hot Water Supply = 70. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Litter filter(s)" (IFCTEXT)
    Opening Range = "0-5 cm" (IFCTEXT)
    Pipes = "Flexible inlet pipe(s)" (IFCTEXT)
    Pressure Loss With Flow 02ls = 250000. (IFCPRESSUREMEASURE) [PASCAL]
    Recognition Range = "60 cm (50 / 60 cm)" (IFCTEXT)
    Spare Parts = "https://www.oras.com/en/products/oras/spareparts/SP6661F/" (IFCTEXT)