IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "Project Number"
Time stamp: "2018-06-20T10:52:56"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20150714_1515(x64) - Exporter 16.2.0.0 - Alternate UI 16.2.0.0"
Application: "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)"

People and organizations
  Person "Paloma" of Organization (no name given)
  Owner history of Person "Paloma" of Organization (no name given) | application "Autodesk Revit 2016 (ENU)" version "2016" identifier "Revit" by Organization "Autodesk Revit 2016 (ENU)" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "Project Number" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 51° 30′ 23.112487″ | longitude -0° 7′ 37.956022″ | elevation above sea level 0.
    IFCBUILDING | postal address: "Enter address here", "London", "London", "United Kingdom"
      IFCBUILDINGSTOREY "Level 0" | long name "Level 0" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "2703F Washbasin faucet, 3 V" | object type "2703F Washbasin faucet, 3 V" | names: "2703F(2013):2703F Washbasin faucet, 3 V:313583" | material: "Brass" | property sets: Pset_ManufacturerTypeInformation, Pset_DistributionFlowElementCommon, Constraints, Dimensions, Identity Data, Mechanical

Types
  IFCVALVETYPE "2703F Washbasin faucet, 3 V" | FAUCET | 1 occurrence | material: "Brass" | property sets: Dimensions, Electrical, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "Project Number" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "2703F(2013): 2703F Washbasin faucet, 3 V" (IFCLABEL)
    Family and Type = "2703F(2013): 2703F Washbasin faucet, 3 V" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "2703F(2013): 2703F Washbasin faucet, 3 V" (IFCLABEL)
    Type Id = "2703F(2013): 2703F Washbasin faucet, 3 V" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: Circle Head - Project Datum" (IFCLABEL)
    Family and Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type = "Level: Circle Head - Project Datum" (IFCLABEL)
    Type Id = "Level: Circle Head - Project Datum" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Oras" (IFCTEXT)
    Category = "Bathroom" (IFCTEXT)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "2703F(2013)" (IFCTEXT)
    Features = "Single lever, battery operated" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "2703F" (IFCTEXT)
    Name = "2703F Washbasin faucet, 3 V" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "Faucet:54x145x163 mm / Hand shower: 57x69x318 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "n/a" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "Circle Head - Project Datum" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "10" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 0" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Class = "Single lever, battery operated" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Group = "Washbasin faucets" (IFCTEXT)
    Manufacturer = "Oras" (IFCTEXT)
    Market = "INT;DNK;EST;FIN;LVA;LTU;NOR;POL;RUS;SWE;UKR" (IFCTEXT)
    Model = "2703F Washbasin faucet, 3 V" (IFCTEXT)
    Name_en = "2703F Washbasin faucet, 3 V" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "2703F" (IFCTEXT)
    Product Datasheet = "https://www.oras.com/datasheet/2703F/en" (IFCTEXT)
    Product Family = "Oras Optima" (IFCTEXT)
    Product URL = "https://www.oras.com/en/products/oras-optima/product/2703F/" (IFCTEXT)
    Type Name = "2703F Washbasin faucet, 3 V" (IFCTEXT)
    URL = "" (IFCTEXT)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Oras" (IFCLABEL)
    ModelReference = "2703F" (IFCLABEL)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "2703F Washbasin faucet, 3 V" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DistanceX-Axis = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    DistanceY-Axis = 100. (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetDefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerDefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 0" (IFCTEXT)
    Level = "Level: Level 0" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0851172864267344 (IFCAREAMEASURE) [SQUARE_METRE]
    Volume = 0.00252068091531427 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    FaucetNominalDepth = 145. (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalHeight = 163. (IFCLENGTHMEASURE) [MILLI METRE]
    FaucetNominalWidth = 54. (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalDepth = 68.5 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalHeight = 317.5 (IFCLENGTHMEASURE) [MILLI METRE]
    HandShowerNominalWidth = 57. (IFCLENGTHMEASURE) [MILLI METRE]
    InletConnectionSize = 10. (IFCLENGTHMEASURE) [MILLI METRE]
    Projection = 98. (IFCLENGTHMEASURE) [MILLI METRE]
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Lead free" (IFCTEXT)
    Extensions = "Rapid popup waste" (IFCTEXT)
    Flow = "Limitation option for maximum flowrate" (IFCTEXT)
    Flow Rate At 300kPa = 0.00423776000657863 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Hand Shower = "Remote operated smart Bidetta" (IFCTEXT)
    Installation Type = "Deck mounted" (IFCTEXT)
    Lever Handle = "Easy grip lever" (IFCTEXT)
    Max Flow Period = 120. (IFCREAL)
    Max. Hot Water Supply = 70. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Pipes = "Flexible inlet pipes" (IFCTEXT)
    Pressure Loss With Flow 01ls = 200000. (IFCPRESSUREMEASURE) [PASCAL]
    Spout Type = "Fixed spout" (IFCTEXT)
    Temperature = "Thermostatic temperature control" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "Anno_Level_Head_Circle: Standard" (IFCLABEL)
    Symbol at End 1 Default = TRUE (IFCBOOLEAN)
    Symbol at End 2 Default = FALSE (IFCBOOLEAN)
  Electrical | properties | on 1 type object
    Battery = "AA 1.5 V Lithium x 2, CR 2450 3 V" (IFCTEXT)
    Number of Devices = "max 8" (IFCTEXT)
    Operating Voltage = 3. (IFCELECTRICVOLTAGEMEASURE) [VOLT]
  General | properties | on 1 type object
    Author = "Convergo AB" (IFCTEXT)
    BIMObjectName = "2703F(2013)" (IFCTEXT)
    ConvergoRefNr = "0087-1806-0085-FI" (IFCTEXT)
    ExpiringDate = "12/2018" (IFCTEXT)
    ManufacterURL = "http://www.oras.com/" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    NBSDescription = "Water supply fittings for washbasins and troughs" (IFCTEXT)
    NBSReference = "45-35-70/371" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_96" (IFCTEXT)
    Uniclass2015Description = "Washbasin manual water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_96" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "13/06/2018" (IFCTEXT)
  Green Building Properties | properties | on 1 type object
    EAN Number = "6414150069963" (IFCTEXT)
    EMC Directive = "2004/108/EY" (IFCTEXT)
    ETA-Danmark = "VA 1.42/20420" (IFCTEXT)
    LVI Number = "6110082" (IFCTEXT)
    NRF Number = "4200054" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Protection Class = "IP 55" (IFCTEXT)
    RSK Number = "8347924" (IFCTEXT)
    STF Certificate = "VTT-RTH-00063-14" (IFCTEXT)
    Sintef Certificate = "Sintef Nr. 3082" (IFCTEXT)
    VVS Number = "704243504" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Text | properties | on 1 type object
    Health Sales Arguments = "Lead free" (IFCTEXT)