IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView_V2.0]"
File name: "0001"
Time stamp: "2023-07-27T17:05:06"
Preprocessor: "The EXPRESS Data Manager Version 5.02.0100.07 : 28 Aug 2013"
Originating system: "20200210_1400(x64) - Exporter 20.2.12.1 - Alternate UI 20.2.12.1"
Application: "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)"

People and organizations
  Person "tpnGSEQT" of Organization (no name given)
  Owner history of Person "tpnGSEQT" of Organization (no name given) | application "Autodesk Revit 2020 (ENU)" version "2020" identifier "Revit" by Organization "Autodesk Revit 2020 (ENU)" | change NOCHANGE | created 1690106945 (2023-07-23T10:09:05Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: SQUARE_METRE
  VOLUMEUNIT: CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  MASSUNIT: KILO GRAM
  MASSDENSITYUNIT: derived
  TIMEUNIT: SECOND
  FREQUENCYUNIT: HERTZ
  THERMODYNAMICTEMPERATUREUNIT: DEGREE_CELSIUS
  THERMALTRANSMITTANCEUNIT: derived
  VOLUMETRICFLOWRATEUNIT: derived
  ELECTRICCURRENTUNIT: AMPERE
  ELECTRICVOLTAGEUNIT: VOLT
  POWERUNIT: WATT
  FORCEUNIT: KILO NEWTON
  ILLUMINANCEUNIT: LUX
  LUMINOUSFLUXUNIT: LUMEN
  LUMINOUSINTENSITYUNIT: CANDELA
  USERDEFINED: derived "Luminous Efficacy"
  LINEARVELOCITYUNIT: derived
  PRESSUREUNIT: PASCAL
  USERDEFINED: derived "Friction Loss"

Spatial structure
IFCPROJECT "0001" | long name "Project Name" | phase "Project Status"
  IFCSITE "Default" | latitude 42° 21′ 31.181945″ | longitude -71° 3′ 24.263305″ | elevation above sea level 0.
    IFCBUILDING
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | object type "Level:8mm Head" | elevation 0.
        contains 1 element
          1 x IFCFLOWCONTROLLER | type IFCVALVETYPE "7140N Bath and shower faucet" | object type "7140N(2023):7140N Bath and shower faucet" | names: "7140N(2023):7140N Bath and shower faucet:427317" | material: "Brass" | property sets: Pset_DistributionFlowElementCommon, Pset_ElementShading, Pset_ManufacturerOccurrence, Pset_ManufacturerTypeInformation, Pset_ProductRequirements, Pset_QuantityTakeOff

Types
  IFCVALVETYPE "7140N Bath and shower faucet" | FAUCET | 1 occurrence | material: "Brass" | property sets: Constraints, Dimensions, General, Green Building Properties, Identity Data, Materials and Finishes

Property sets
  Other(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family Name = "Level" (IFCTEXT)
  Identity Data(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Type Name = "8mm Head" (IFCTEXT)
  Pset_DistributionFlowElementCommon | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "7140N Bath and shower faucet" (IFCIDENTIFIER)
  Pset_ElementShading | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Color = "Chrome" (IFCLABEL)
  Pset_ManufacturerOccurrence | properties | on 1 object (1 IFCFLOWCONTROLLER)
    BarCode = "n/a" (IFCIDENTIFIER)
    SerialNumber = "n/a" (IFCIDENTIFIER)
  Pset_ManufacturerTypeInformation | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Manufacturer = "Oras" (IFCLABEL)
    ModelReference = "7140N" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Name = "7140N Bath and shower faucet" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Name = "Level 1" (IFCLABEL)
  Pset_ProductRequirements | properties | on 1 object (1 IFCBUILDING)
    Category = "Project Information" (IFCLABEL)
  Pset_QuantityTakeOff | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Reference = "7140N Bath and shower faucet" (IFCIDENTIFIER)
  Constraints | properties | on 1 object (1 IFCFLOWCONTROLLER)
    DefaultElevation = 900. (IFCLENGTHMEASURE) [MILLI METRE]
    Elevation from Level = 0. (IFCLENGTHMEASURE) [MILLI METRE]
    Host = "Level : Level 1" (IFCTEXT)
    Level = "Level: Level 1" (IFCLABEL)
    Offset from Host = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 type object
    Default Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Area = 0.0915002015990934 (IFCAREAMEASURE) [SQUARE_METRE]
    ConnectorDirection = 0 (IFCINTEGER)
    ConnectorDirectionNote = "0-Up II 1-Back II 2-Down" (IFCTEXT)
    InletConnectionSize = 15. (IFCLENGTHMEASURE) [MILLI METRE]
    InletDistance = 150. (IFCLENGTHMEASURE) [MILLI METRE]
    OutletAngle = 0. (IFCPLANEANGLEMEASURE) [DEGREE (conversion based)]
    Volume = 0.00361650225379756 (IFCVOLUMEMEASURE) [CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 type object
    NominalDepth = 168.172583364881 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalHeight = 62.6469725943131 (IFCLENGTHMEASURE) [MILLI METRE]
    NominalWidth = 342.094022151003 (IFCLENGTHMEASURE) [MILLI METRE]
  Identity Data | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Author = "" (IFCTEXT)
    Building Name = "" (IFCTEXT)
    Organization Description = "" (IFCTEXT)
    Organization Name = "" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Mark = "2" (IFCTEXT)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCTEXT)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 type object
    2D/3D/BIM Files URL = "http://static.oras.com/bim/7140N" (IFCTEXT)
    3D View = "https://static.oras.com/AR/7140N" (IFCTEXT)
    Assembly Code = "" (IFCTEXT)
    Assembly Description = "" (IFCTEXT)
    Catalog Drawing URL = "http://static.oras.com/catdrw/7140N" (IFCTEXT)
    Code Name = "" (IFCTEXT)
    Description = "" (IFCTEXT)
    Dimension Drawing URL = "http://static.oras.com/dimdrw/7140N" (IFCTEXT)
    FDV Document URL = "http://www.oras.com/datasheet/7140N/en/fdv" (IFCTEXT)
    Flow Drawing URL = "http://static.oras.com/flowchart/7140N" (IFCTEXT)
    Group = "Bath and shower faucet" (IFCTEXT)
    Installation and Maintenance Guide URL = "http://static.oras.com/manual/7140N" (IFCTEXT)
    Interactive AR View URL = "https://static.oras.com/AR/7140N" (IFCTEXT)
    Manufacturer = "Oras" (IFCTEXT)
    Market = "International;Norway;Sweden;Denmark" (IFCTEXT)
    Mobile Product Information URL = "http://mpi.oras.com/7140N" (IFCTEXT)
    Model = "7140N Bath and shower faucet" (IFCTEXT)
    Name_en = "7140N Bath and shower faucet" (IFCTEXT)
    OmniClass Number = "23.45.55.00" (IFCTEXT)
    OmniClass Title = "Sanitary Faucets, Wastes" (IFCTEXT)
    Product Code = "7140N" (IFCTEXT)
    Product Family = "Oras Optima" (IFCTEXT)
    Product Image URL = "http://static.oras.com/image/7140N" (IFCTEXT)
    Product URL = "http://static.oras.com/7140N" (IFCTEXT)
    Technical DataSheet URL = "http://www.oras.com/datasheet/7140N/en" (IFCTEXT)
    Type Name = "7140N Bath and shower faucet" (IFCTEXT)
    URL = "" (IFCTEXT)
    Warranty Information URL = "http://warranty.oras.com" (IFCTEXT)
  Mechanical | properties | on 1 object (1 IFCFLOWCONTROLLER)
    System Abbreviation = "" (IFCTEXT)
    System Classification = "Domestic Hot Water,Domestic Cold Water" (IFCTEXT)
    System Name = "" (IFCTEXT)
  Mechanical | properties | on 1 type object
    Advanced Features = "Inner body made of DZR brass" (IFCTEXT)
    Backflow Prevention EN1717 = "EB" (IFCTEXT)
    Connection = "Direct connection;Internal thread" (IFCTEXT)
    Connection Size = "G3/4" (IFCTEXT)
    Diverter = "Turn operated diverter;Integrated into flow control handle" (IFCTEXT)
    Eco Flow At 300kPa = 0.00423776000657863 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Excluded Items = "Without couplings" (IFCTEXT)
    Flow Rate At 300kPa = 0.0113006933508763 (IFCVOLUMETRICFLOWRATEMEASURE) [derived]
    Installation Type = "Wall mounted" (IFCTEXT)
    Installation Width = "CC150± 3 mm" (IFCTEXT)
    Lever Handle = "Temperature control handle;Flow control handle;Hot/Cold symbols;Easy-Grip surface;Eco feature for water flow" (IFCTEXT)
    Max. Hot Water Supply = 80. (IFCTHERMALTRANSMITTANCEMEASURE) [derived]
    Mechanical Parts = "Ceramic head part for flow control;Thermostatic cartridge for automatic temperature control;Non-return valve(s);Litter filter(s)" (IFCTEXT)
    Pressure Loss With Flow 03ls = 265000. (IFCPRESSUREMEASURE) [PASCAL]
    Shower Parts = "MagShelf" (IFCTEXT)
    Spout Projection = "131 mm" (IFCTEXT)
    Spout Type = "Fixed spout" (IFCTEXT)
    Surface treatment = "Chrome" (IFCTEXT)
    Temperature Adjustments = "Safety stop against scalding at 38°C;The housing of the fittings conducts minimal heat" (IFCTEXT)
    Working Pressure = "100 - 1000 kPa" (IFCTEXT)
  Other | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    Category = "Project Information" (IFCLABEL)
    Client Name = "Owner" (IFCTEXT)
    Project Address = "Enter address here" (IFCTEXT)
    Project Issue Date = "Issue Date" (IFCTEXT)
    Project Name = "Project Name" (IFCTEXT)
    Project Number = "0001" (IFCTEXT)
    Project Status = "Project Status" (IFCTEXT)
  Other | properties | on 1 object (1 IFCFLOWCONTROLLER)
    AssetIdentifier = "n/a" (IFCTEXT)
    Barcode = "n/a" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    Family = "7140N(2023): 7140N Bath and shower faucet" (IFCLABEL)
    Family and Type = "7140N(2023): 7140N Bath and shower faucet" (IFCLABEL)
    InstallationDate = "n/a" (IFCTEXT)
    SerialNumber = "n/a" (IFCTEXT)
    TagNumber = "n/a" (IFCTEXT)
    Type = "7140N(2023): 7140N Bath and shower faucet" (IFCLABEL)
    Type Id = "7140N(2023): 7140N Bath and shower faucet" (IFCLABEL)
    WarrantyStartDate = "n/a" (IFCTEXT)
  Other | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Category = "Levels" (IFCLABEL)
    Family = "Level: 8mm Head" (IFCLABEL)
    Family and Type = "Level: 8mm Head" (IFCLABEL)
    Type = "Level: 8mm Head" (IFCLABEL)
    Type Id = "Level: 8mm Head" (IFCLABEL)
  Other | properties | on 1 type object
    AccessibilityPerformance = "n/a" (IFCTEXT)
    AssetType = "Fixed" (IFCTEXT)
    Brand = "Oras" (IFCTEXT)
    Category = "Plumbing Fixtures" (IFCLABEL)
    CodePerformance = "n/a" (IFCTEXT)
    Color = "Chrome" (IFCTEXT)
    Constituents = "n/a" (IFCTEXT)
    DurationUnit = "Year" (IFCTEXT)
    ExpectedLife = "n/a" (IFCTEXT)
    Family Name = "7140N(2023)" (IFCTEXT)
    Features = "Thermostatic" (IFCTEXT)
    Finish = "Polished" (IFCTEXT)
    Grade = "n/a" (IFCTEXT)
    Material = "Brass/Plastic" (IFCTEXT)
    ModelNumber = "n/a" (IFCTEXT)
    ModelReference = "7140N" (IFCTEXT)
    Name = "7140N Bath and shower faucet" (IFCTEXT)
    ReplacementCost = "n/a" (IFCTEXT)
    Shape = "Sculptured" (IFCTEXT)
    Size = "345x170x65 mm" (IFCTEXT)
    SustainabilityPerformance = "n/a" (IFCTEXT)
    WarrantyDescription = "http://warranty.oras.com" (IFCTEXT)
    WarrantyDurationLabor = "n/a" (IFCTEXT)
    WarrantyDurationParts = "n/a" (IFCTEXT)
    WarrantyDurationUnit = "Year" (IFCTEXT)
    WarrantyGuarantorLabor = "n/a" (IFCTEXT)
    WarrantyGuarantorParts = "n/a" (IFCTEXT)
  Phasing | properties | on 1 object (1 IFCFLOWCONTROLLER)
    Phase Created = "New Construction" (IFCLABEL)
  General | properties | on 2 objects (1 IFCBUILDING, 1 IFCSITE)
    NBLProjectId = "8b2fe5c3-633f-4129-b12a-2a6d73f37baa" (IFCTEXT)
    NBSSpecificationPath = "" (IFCTEXT)
  General | properties | on 1 type object
    Author = "BIMStone" (IFCTEXT)
    BIMObjectName = "7140N(2023)" (IFCTEXT)
    ManufacturerName = "Oras" (IFCTEXT)
    ManufacturerURL = "http://www.oras.com" (IFCTEXT)
    NBSDescription = "Shower mixers" (IFCTEXT)
    NBSReference = "45-35-70/335" (IFCTEXT)
    ProductInformation = "n/a" (IFCTEXT)
    Revision = "n/a" (IFCTEXT)
    Uniclass2 = "Pr_40_30_96_81" (IFCTEXT)
    Uniclass2015Description = "Shower thermostatic water supply sets" (IFCTEXT)
    Uniclass2015Reference = "Pr_40_20_87_81" (IFCTEXT)
    Version = "1" (IFCTEXT)
    VersionDate = "01/06/2023" (IFCTEXT)
  Pset_AirSideSystemInformation | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  Pset_BuildingStoreyCommon | properties | on 1 object (1 IFCBUILDINGSTOREY)
    AboveGround = UNKNOWN (IFCLOGICAL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    IsLandmarked = UNKNOWN (IFCLOGICAL)
    NumberOfStoreys = 1 (IFCINTEGER)
  Constraints(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = "Project Base Point" (IFCIDENTIFIER)
  Graphics(Type) | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Centre" (IFCLABEL)
    Line Weight = "1" (IFCIDENTIFIER)
    Symbol = "M_Level Head - Circle: M_Level Head - Circle" (IFCLABEL)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Green Building Properties | properties | on 1 type object
    EAN Number = "6414150099441" (IFCTEXT)
    EN Standard = "EN1111" (IFCTEXT)
    ETIM Class Number = "EC010862 Bath mixing tap" (IFCTEXT)
    Noise Class 03ls = "I (ISO 3822)" (IFCTEXT)
    Noise Class = "I (ISO 3822)" (IFCTEXT)
    Sales Package dimensions (LxWxH) = "359 x 212 x 75" (IFCTEXT)
    UNSPSC Class Number = "30181700 Faucets or taps" (IFCTEXT)
    URL Declaration Of Performance (DOP) = "http://static.oras.com/doc/DoP" (IFCTEXT)
    URL Declaration of Asbestos = "http://static.oras.com/doc/asbestos" (IFCTEXT)
    URL Declaration of Conformity = "http://static.oras.com/DoC/7140N" (IFCTEXT)
    URL Declaration of SCIP = "http://static.oras.com/doc/SCIP" (IFCTEXT)
    URL EU Packaging Declaration = "http://static.oras.com/doc/packaging" (IFCTEXT)
    URL EcoLabel Declaration = "http://static.oras.com/doc/EcoLabel" (IFCTEXT)
    URL REACH = "http://static.oras.com/doc/reach" (IFCTEXT)
    URL UWL = "http://static.oras.com/UWL/7140N" (IFCTEXT)
  Materials and Finishes | properties | on 1 type object
    FaucetMainMaterial = "Brass" (IFCLABEL)
  Pset_ValveTypeCommon | properties | on 1 type object
    CloseOffRating = 0. (IFCPRESSUREMEASURE) [PASCAL]
    FlowCoefficient = 0. (IFCREAL)
    ValveMechanism in {"n/a"} (IFCLABEL)
    ValveOperation in {"n/a"} (IFCLABEL)
    ValvePattern in {"n/a"} (IFCLABEL)
  Pset_ValveTypeFaucet | properties | on 1 type object
    Finish = "Polished" (IFCTEXT)

Other addresses and roles
  2 x postal address: "Enter address here", "Boston", "MA"